CeramillMotion Remote-Control Example Application

Description: Example showing how to remotely control the CeramillMotion Appliacation EST1274
Author     : Günter Marte, Amann Girrbach AG
Documents  : EDA0021
Hardware   : PC with Windows >= Windows XP, .NET-Framewortk >= 3.5


===============================================================================    
Change Log
=============================================================================== 

EST1280-01  G. Marte, 2013-02-26
----------

1. Instance of member variable m_S1274 is created in the constructor, message on exeption.


EST1280-02  G. Marte, 2013-05-25
----------

1. Ecxeption message if connection to CeramillMotion failed.


EST1280-03  G. Marte, 2017-02-14
----------

1. Alternative communication via file I/O available (requires EST1274-49.00 or later)

2. Available standard commands are read from file CeramillMotionRemoteControl.Commands.txt.


EST1280-04  G. Marte, 2017-04-10
----------

1. New Commands added to CeramillMotionRemoteControl.Commands.txt.


EST1280-05  G. Marte, 2017-06-26
----------

1.  File I/O extension added

    You can optionally add an extension for the execute and result files - e. g. execute-123 and result-123
    This is useful if two or more remote controllers are involved to control the CeramillMotion Application.
    The first remote controller can write/read the files execute1 and result1, the second one uses execute2 and result2...
    This feature is supported for CeramillMotion EST1274-49.12 or newer.